***************************************************************
      Roland METAZA DRIVER for Windows(R) XP
***************************************************************

We do recommend you to read through this document first for your better understanding of Roland METAZA DRIVER. This "Readme" file provides some important information to install DRIVER.

Explanation here is assuming that you are already familiar with operations on Windows. The further information about operation on Windows, please refer the user's manual from Microsoft Corp.

If you are reading this file with Notepad, check 'WordWrap' in Edit menu so that you can read more easily.


< Table of Contents >

1. In the beginning 
2. Supported Models
3. Installing the Driver
4. Uninstalling the Driver
5. Important Notes


* "Windows(R)" is registered trademark or trademark of Microsoft(R) Corporation in the United States and/or other countries.

Copyright (C) 2002-2010 Roland DG Corporation


----------------------------------------

< 1. In the beginning >

This driver provides you the capability to output printing to the Roland METAZA machine from your Windows application software.


----------------------------------------

< 2. Supported Models >

- METAZA MPX-90
- METAZA MPX-80
- METAZA MPX-70
- METAZA MPX-60
- METAZA MPX-50


----------------------------------------

< 3. Installing the Driver >

-	When connected to a [COM] or [LPT] port

*	Log on as administrator or as a member of the Administrators group.
*	If an older version of the driver is installed, uninstall it before you install the new one. For more information about how to remove the driver, refer to the next section, "Uninstalling the Driver."
*	If the message [Digital Signature Not Found] appears during installation, click [Yes].

1.	Switch off the power to the machine, then detach the connector cable between the machine and the computer.
2.	Turn on the computer. After Windows has started, turn on the machine. At this time, do not attach the connector cable to the computer and the machine yet.
3.	From the [Start] menu, select [Run], then click [Browse].
4.	From the [File Locations] list, choose the name of the drive or folder where the driver is located.
5.	Select "SETUP.EXE" and click [Open], then click [OK].
6.	The Setup program for the driver starts.
7.	Click [Install] to choose it.
	Choose the machine and connection port you're using, then click [Start]. 
8.	After installation has finished, use the cable to make the connection between the computer and the machine.
	For a USB connection, attaching the cable and turning on the machine enables the driver.

-	When connected to a [USB] port

*	Log on as administrator or as a member of the Administrators group.
*	If an older version of the driver is installed, uninstall it before you install the new one. For more information about how to remove the driver, refer to the next section, "Uninstalling the Driver."
*	During installation, if a message that the Windows Logo test was not passed appears, click [Continue Anyway].

1.	Switch off the power to the machine, then detach the connector cable between the machine and the computer.
2.	Turn on the computer. After Windows has started, turn on the machine. 
3.	Use the cable to connect the computer and the machine.
	The [Found New Hardware Wizard] appears.
4.	When the screen shown "Can Windows connect to Windows Update to search for software?", select [No, not this time], then click [Next].
	If the screen does not appear, refer to step 5.
5.	Select [Install from a list or specific location], then click [Next].
6.	Click [Browse].
7.	From the [Browse Folders] list, select the name of the drive or folder where the driver is located, then click [OK].
8.	Click [Next].
9.	Click [Finish] to finish installation.


----------------------------------------

< 4. Uninstalling the Driver >

*	Log on as administrator or as a member of the Administrators group.

1.	Switch off the power to the machine, then detach the connector cable between the machine and the computer.
2.	Start Windows.
3.	From the [Start] menu, select [Settings], then choose [Printers and Faxes] (or [Printers]).
4.	Click the driver for the machine to delete to select it, then go to [File] and select [Delete].
5.	A message prompting you to confirm deletion appears. Click [Yes].
6.	Go to [File] and select [Server Properties].
7.	Click the [Driver] tab, then from the [Installed printer drivers] list, choose the machine to delete.
8.	Click [Delete]. When the prompt message appears, click [Yes].
9.	From the [Start] menu, select [Run], then click [Browse].
10.	From the [File Locations] list, choose the name of the drive or folder where the driver is located. (*)
11.	Select "SETUP.EXE" and click [Open], then click [OK].
12.	The Setup program for the driver starts.
13.	Click [Uninstall] to choose it.
	Select the machine to delete, then click [Start].
14.	If it is necessary to restart your computer, a window prompting you to restart it appears. Click [Yes].
15.	The uninstallation finishes after the computer restarts.


(*) When using the CD-ROM, specify the folder as shown below (assuming your CD-ROM drive is the D drive).

	D:\Drivers\WINXPX86

If you're not using the CD-ROM, go to the Roland DG Corp. website (http://www.rolanddg.com/) and download the driver for the machine you want to delete, then specify the folder where you want to expand the downloaded file.


----------------------------------------

< 5. Important Notes >

- This driver does not support [Test Print].


========================================================

If you have further questions or problem, please contact to your local vendor or Roland sales center.
